PRISM_DATASET_FILENAME: cai_tmin_us_us_30s_201601.bil, cai_tmin_us_us_30s_201602.bil, cai_tmin_us_us_30s_201603.bil, cai_tmin_us_us_30s_201604.bil, cai_tmin_us_us_30s_201605.bil, cai_tmin_us_us_30s_201606.bil, cai_tmin_us_us_30s_201607.bil, cai_tmin_us_us_30s_201608.bil, cai_tmin_us_us_30s_201609.bil, cai_tmin_us_us_30s_201610.bil, cai_tmin_us_us_30s_201611.bil, cai_tmin_us_us_30s_201612.bil
PRISM_DATASET_CREATE_DATE: 20160825, 20160825, 20160912, 20161012, 20161114, 20161208, 20170112, 20170215, 20170316, 20170411, 20170411, 20170615
PRISM_DATASET_TYPE: an81/r1503
PRISM_DATASET_VERSION: M2
PRISM_CODE_VERSION: 16.1-20161010-1224, 16.1-20161010-1224, 16.1-20161010-1224, 16.1-20161010-1224, 16.1-20161010-1224, 16.1-20161010-1224, 16.1-20161010-1224, 16.1-20161010-1224, 16.1-20161010-1224, 16.1-20161010-1224, 16.1-20161010-1224, 16.1-20170524-1355
PRISM_DATASET_REMARKS: This grid was developed in three steps:  (1) temperature was initially modeled with PRISM at 30-arc-second (~800-m) resolution for each month of the year to produce the source grids listed under PRISM_FILENAME, on the date(s) listed under PRISM_CREATE_DATE; (2) these twelve 800-m grids were upscaled to 2.5-arc-minute (~4-km) resolution with a Gaussian filter; and (3) the resulting twelve 4-km grids were averaged to obtain a 4-km annual grid.
