PRISM_DATASET_FILENAME: prism_solslope_us_25m_2012.tif
PRISM_DATASET_CREATE_DATE: 20260310-1023
PRISM_SOURCE_FILENAME: topo_gsolar_slope_us_us_30s_201201.bil, topo_gsolar_slope_us_us_30s_201202.bil, topo_gsolar_slope_us_us_30s_201203.bil, topo_gsolar_slope_us_us_30s_201204.bil, topo_gsolar_slope_us_us_30s_201205.bil, topo_gsolar_slope_us_us_30s_201206.bil, topo_gsolar_slope_us_us_30s_201207.bil, topo_gsolar_slope_us_us_30s_201208.bil, topo_gsolar_slope_us_us_30s_201209.bil, topo_gsolar_slope_us_us_30s_201210.bil, topo_gsolar_slope_us_us_30s_201211.bil, topo_gsolar_slope_us_us_30s_201212.bil
PRISM_SOURCE_CREATE_DATE: 20251120-1428, 20251120-1428, 20251120-1428, 20251120-1428, 20251120-1428, 20251120-1428, 20251120-1428, 20251120-1428, 20251120-1428, 20251120-1428, 20251120-1428, 20251120-1428
PRISM_DATASET_TYPE: an91/r2112
PRISM_DATASET_VERSION: M3
PRISM_CODE_VERSION: 16.2-20250715-1813
PRISM_DATASET_RELEASE_NUMBER: 2
PRISM_DATASET_REMARKS: This grid was developed in three steps: (1) solar data were modeled with PRISM at 30-arc-second (~800m) resolution to produce the source grid(s) listed under PRISM_SOURCE_FILENAME, on the date(s) listed under PRISM_SOURCE_CREATE_DATE; (2) These twelve monthly 800m grids were then upscaled to 2.5-arc-minute(~ 4km) resolution with a Gaussian filter; and (3) The resulting twelve monthly 4km grids were averaged to obtain a 4km mean annual solar grid.
