PRISM_DATASET_FILENAME: prism_solslope_us_25m_1992.tif
PRISM_DATASET_CREATE_DATE: 20260310-1023
PRISM_SOURCE_FILENAME: topo_gsolar_slope_us_us_30s_199201.bil, topo_gsolar_slope_us_us_30s_199202.bil, topo_gsolar_slope_us_us_30s_199203.bil, topo_gsolar_slope_us_us_30s_199204.bil, topo_gsolar_slope_us_us_30s_199205.bil, topo_gsolar_slope_us_us_30s_199206.bil, topo_gsolar_slope_us_us_30s_199207.bil, topo_gsolar_slope_us_us_30s_199208.bil, topo_gsolar_slope_us_us_30s_199209.bil, topo_gsolar_slope_us_us_30s_199210.bil, topo_gsolar_slope_us_us_30s_199211.bil, topo_gsolar_slope_us_us_30s_199212.bil
PRISM_SOURCE_CREATE_DATE: 20260123-0909, 20260123-0910, 20260123-0910, 20260123-0910, 20260123-0910, 20260123-0910, 20260123-0911, 20260123-0911, 20260123-0911, 20260123-0911, 20260123-0911, 20260123-0912
PRISM_DATASET_TYPE: an91/r2112
PRISM_DATASET_VERSION: M3
PRISM_CODE_VERSION: 16.2-20250715-1813
PRISM_DATASET_RELEASE_NUMBER: 2
PRISM_DATASET_REMARKS: This grid was developed in three steps: (1) solar data were modeled with PRISM at 30-arc-second (~800m) resolution to produce the source grid(s) listed under PRISM_SOURCE_FILENAME, on the date(s) listed under PRISM_SOURCE_CREATE_DATE; (2) These twelve monthly 800m grids were then upscaled to 2.5-arc-minute(~ 4km) resolution with a Gaussian filter; and (3) The resulting twelve monthly 4km grids were averaged to obtain a 4km mean annual solar grid.
