PRISM_DATASET_FILENAME: prism_soltotal_us_25m_1981.tif
PRISM_DATASET_CREATE_DATE: 20260310-1220
PRISM_SOURCE_FILENAME: topo_gsolar_total_us_us_30s_198101.bil, topo_gsolar_total_us_us_30s_198102.bil, topo_gsolar_total_us_us_30s_198103.bil, topo_gsolar_total_us_us_30s_198104.bil, topo_gsolar_total_us_us_30s_198105.bil, topo_gsolar_total_us_us_30s_198106.bil, topo_gsolar_total_us_us_30s_198107.bil, topo_gsolar_total_us_us_30s_198108.bil, topo_gsolar_total_us_us_30s_198109.bil, topo_gsolar_total_us_us_30s_198110.bil, topo_gsolar_total_us_us_30s_198111.bil, topo_gsolar_total_us_us_30s_198112.bil
PRISM_SOURCE_CREATE_DATE: 20260123-0846, 20260123-0846, 20260123-0846, 20251120-1421, 20251120-1421, 20251120-1421, 20251120-1421, 20260123-0846, 20260123-0846, 20260123-0847, 20260123-0847, 20251120-1421
PRISM_DATASET_TYPE: an91/r2112
PRISM_DATASET_VERSION: M3
PRISM_CODE_VERSION: 16.2-20250715-1813
PRISM_DATASET_RELEASE_NUMBER: 2
PRISM_DATASET_REMARKS: This grid was developed in three steps: (1) solar data were modeled with PRISM at 30-arc-second (~800m) resolution to produce the source grid(s) listed under PRISM_SOURCE_FILENAME, on the date(s) listed under PRISM_SOURCE_CREATE_DATE; (2) These twelve monthly 800m grids were then upscaled to 2.5-arc-minute(~ 4km) resolution with a Gaussian filter; and (3) The resulting twelve monthly 4km grids were averaged to obtain a 4km mean annual solar grid.
